{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Ａシート　アルミ樹脂複合 記入例","Ａシート　アルミPG 記入例","Ａシート　樹脂 記入例","プルダウン項目 (2)","マスターシート","DATA BASE","建具仕様番号"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":17,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Ａシート　アルミ樹脂複合 記入例","index":0,"n_rows":50,"n_cols":32,"rows_kept":50,"cut":false,"hidden":false,"merged":[[0,28,0,31],[1,29,1,31],[2,17,2,18],[2,19,2,24],[2,26,2,31],[3,23,4,27],[3,28,4,29],[3,30,4,31],[4,1,5,7],[5,8,8,9],[5,10,5,12],[5,13,6,18],[5,19,8,22],[5,23,8,27],[5,28,8,29],[3,1,3,5],[3,8,4,9],[3,10,3,12],[3,13,4,18],[3,19,4,22],[5,30,8,31],[6,1,6,5],[7,1,8,7],[7,10,7,12],[7,13,7,18],[8,10,8,12],[8,13,8,18],[9,8,9,9],[10,11,12,11],[10,12,11,12],[10,13,15,13],[10,14,11,17],[14,8,15,8],[14,9,15,9],[14,10,15,10],[10,30,15,30],[10,31,15,31],[11,1,15,1],[11,2,15,2],[11,3,15,3],[11,4,15,4],[11,5,15,5],[11,6,15,6],[10,18,15,18],[12,20,12,23],[12,24,13,25],[12,26,13,29],[13,11,15,11],[13,20,15,20],[13,21,15,21],[13,22,15,22],[14,26,15,26],[12,12,15,12],[12,14,15,14],[12,15,15,15],[12,16,15,16],[12,17,15,17],[12,19,15,19],[14,27,15,27],[14,28,15,28],[14,29,15,29],[16,1,16,2],[16,7,16,9],[16,14,16,17],[16,19,16,23],[16,26,16,28],[11,7,15,7],[11,8,11,10],[11,24,11,29],[12,8,13,10],[10,19,11,23],[10,24,10,29],[13,23,15,23],[14,25,15,25],[45,7,45,9],[45,26,45,31],[48,1,49,4],[38,1,38,31],[39,1,39,2],[39,7,39,9],[39,12,39,13],[39,14,39,18],[39,19,39,23],[39,26,39,28]]}
[]
[null,"外部開口部リスト２０２１年版 （兼 製品保証及び納入明細書）",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"記入例【アルミ樹脂複合】",null,null,null,null,null,null,null,null,null,null,"〔NO．　／　〕"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"現場納入日",null,"〇〇〇〇年〇〇月〇〇日",null,null,null,null,null,"取付確認日","〇〇〇〇年〇〇月〇〇日"]
[null,"物件の名称",null,null,null,null,null,null,"地域区分",null,"販売店名(代表者名）",null,null,"株式会社 〇〇サッシ販売",null,null,null,null,null,"取扱い事業所",null,null,null,"組立事業所登録NO.",null,null,null,null,"施工（管理）者　　　　　　　　　　　　　　　　　　　　　　",null,"納入確認者　　　　　　　　　　　　　　　　"]
[null,"〇△様邸 新築工事"]
[null,null,null,null,null,null,null,null,6,null,"取扱い事業所名",null,null,"株式会社 〇〇サッシ販売　△△営業所",null,null,null,null,null,"印",null,null,null,"１３－〇〇〇〇",null,null,null,null,"印",null,"印"]
[null,"物件の所在地 （又は地番）"]
[null,"〇〇県××市△△　〇丁目△番地×号",null,null,null,null,null,null,null,null,"事業所住所",null,null,"〇〇県△△市××　１２３－４"]
[null,null,null,null,null,null,null,null,null,null,"TEL",null,null,"０１２３-４５-６７８９"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"記入区分","建具　　　　　　　　　　　　　　仕様","　※１参照（サッシ協ＨＰ）","ガラス仕様 　厚さ・種類　　　　　　　　　　　　　　　　　〔①～④各項目を全て記入〕",null,null,null,"　※2参照（サッシ協ＨＰ）","付属部材",null,null,null,null,"住宅性能表示制度の必須項目",null,null,null,null,null,"　　サッシメーカー","　　シリーズ名又は記号"]
[null,"設置階","部位（部屋）","建具番号（窓番）","方位","窓・ドア区分","開閉形式","サイズ呼称","開口面積",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"温熱環境・エネルギー消費量"]
[null,null,null,null,null,null,null,null,"※外法寸法　　　　　　　　　　　　　　　　　　　　　（小数点第2位まで）",null,null,null,"種類",null,"①ガラス種類","②Ｌｏｗ－Ｅの有無","③中空層種類","④中空層厚み",null,"なし","あり",null,null,null,"熱貫流率\n　U値\n［W/㎡K］",null,"日射熱取得率  \nη値"]
[null,null,null,null,null,null,null,null,null,null,null,"仕様　　　　　　　　　　　　　　　　　　　　　　又は　　　　　　　計算　　　　　　　　　　（試験）",null,null,null,null,null,null,null,null,"シャッター・雨戸","和障子","風除室","外付ブラインド"]
[null,null,null,null,null,null,null,null,"外法　　 W　　　　（㎜）","外法　　　　　H　　　　　  （㎜）","W×H　　　（㎡）",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"性能根拠","付属\n部材\nなし","和障子","外付　　　　　　　　　　　　ブラインド","性能根拠"]
[]
[null,"選  択",null,"直接記入","選  択","選  択","選     択","直接記入",null,null,"自動表記","選  択","選     択","自動表記","選     択",null,null,null,"自動表記","選     択",null,null,null,null,"自動表記/直接入力","自動表記","自動表記/直接入力",null,null,"自動表記","選   択","直接記入"]
[1,"１階","リビング","ＡＷ-1","南","一重窓","引違い","16520",1690,2030,{"$f":"I18*J18/1000000","v":3.4306999999999999},"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M18,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,{"$f":"GLASS_SPEC5(N18,O18,P18,Q18,R18,\"マスターシート!A3:F433\")","v":78},"○","　","　","　","　",{"$f":"VALUE_U_ETA_P(N18,S18,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.91},{"$f":"VLOOKUP(L18,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},{"$f":"VALUE_U_ETA(T18,N18,S18,\"DATA BASE\",\"A\",\"F\",\"H3:H433\")","v":0.51},{"$f":"VALUE_U_ETA_2(V18,X18,N18,S18,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},{"$f":"VALUE_U_ETA(X18,N18,S18,\"DATA BASE\",\"A\",\"F\",\"J3:J433\")","v":""},{"$f":"VLOOKUP(L18,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[2,"１階","リビング","ＡＷ-2","南","一重窓","引違い","16520",1690,2030,{"$f":"I19*J19/1000000","v":3.4306999999999999},"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M19,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,{"$f":"GLASS_SPEC5(N19,O19,P19,Q19,R19,\"マスターシート!A3:F433\")","v":78},"○","　",null,null,null,{"$f":"VALUE_U_ETA_P(N19,S19,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.91},{"$f":"VLOOKUP(L19,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},{"$f":"VALUE_U_ETA(T19,N19,S19,\"DATA BASE\",\"A\",\"F\",\"H3:H433\")","v":0.51},{"$f":"VALUE_U_ETA_2(V19,X19,N19,S19,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},"",{"$f":"VLOOKUP(L19,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[3,"１階","和室","ＡＷ-3","南","一重窓","引違い","25620",2600,2030,5.2779999999999996,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M20,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　",null,null,null,{"$f":"VALUE_U_ETA_P(N20,S20,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.91},{"$f":"VLOOKUP(L20,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},{"$f":"VALUE_U_ETA(T20,N20,S20,\"DATA BASE\",\"A\",\"F\",\"H3:H433\")","v":0.51},{"$f":"VALUE_U_ETA_2(V20,X20,N20,S20,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},"",{"$f":"VLOOKUP(L20,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[4,"２階","寝室","ＡＷ-4","南","一重窓","引違い","16509",1690,970,1.6393,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M21,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"　","　","○","　",null,{"$f":"VALUE_U_ETA_P(N21,S21,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.91},{"$f":"VLOOKUP(L21,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"",0.3,"",{"$f":"VLOOKUP(L21,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[5,"２階","子供室","ＡＷ-5","南","一重窓","引違い","16520",1690,2030,3.4306999999999999,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M22,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　",null,"　","　",{"$f":"VALUE_U_ETA_P(N22,S22,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.91},{"$f":"VLOOKUP(L22,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L22,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[6,"２階","子供室","ＡＷ-6","南","一重窓","引違い","16520",1690,2030,3.4306999999999999,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M23,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L23,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L23,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[7,"１階","トイレ","ＡＷ-7","北","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M24,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L24,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L24,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[8,"１階","洗面所","ＡＷ-8","北","一重窓","たてすべり出し","06009",640,970,0.62080000000000002,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M25,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L25,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L25,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[9,"１階","ホール","ＡＷ-9","北","一重窓","ＦＩＸ","02611",300,1170,0.35099999999999998,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M26,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L26,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L26,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[10,"２階","ホール","ＡＷ-10","北","一重窓","ＦＩＸ","02609",300,970,0.29099999999999998,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M27,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L27,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L27,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[11,"１階","トイレ","ＡＷ-11","北","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M28,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",15,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L28,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L28,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[12,"１階","リビング","ＡＷ-12","東","一重窓","引違い","16511",1690,1170,1.9773000000000001,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M29,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L29,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L29,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[13,"１階","キッチン","ＡＷ-13","東","一重窓","引違い","11907",1235,770,0.95094999999999996,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M30,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",15,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L30,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L30,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[14,"２階","子供室","ＡＷ-14","東","一重窓","たてすべり出し","06009",640,970,0.62080000000000002,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M31,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L31,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L31,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[15,"１階","浴室","ＡＷ-15","西","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M32,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",15,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L32,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L32,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[16,"２階","寝室","ＡＷ-16","西","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M33,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L33,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L33,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[17,"２階","クローゼット","ＡＷ-17","西","一重窓","たてすべり出し","06009",640,970,0.62080000000000002,"仕様","アルミ樹脂複合",{"$f":"VLOOKUP(M34,'プルダウン項目 (2)'!M27:N42,2,0)","v":2},"複層","LowE（日射取得型）","A",16,78,"○","　","　","　","　",2.91,{"$f":"VLOOKUP(L34,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.51,"","",{"$f":"VLOOKUP(L34,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＡＪサッシ"]
[]
[]
[]
[]
[null,"◎以下の行は直接入力です。"]
[null,"選  択",null,"直接記入","選  択","選  択","選   択","直接記入",null,null,"自動表記","直接記入","直接記入",null,"直接記入",null,null,null,null,"選   択",null,null,null,null,"直接記入","直接記入","直接記入",null,null,"直接記入","選  択","直接記入"]
[22,"１階","玄関","ＡＷ-18","西","ドア","玄関ドア","06009",640,970,{"$f":"I41*J41/1000000","v":0.62080000000000002},"計算/試験","ドア",{"$f":"VLOOKUP(M41,'プルダウン項目 (2)'!M27:N42,2,0)","v":7},"ガラス無し","無し","N","無し",{"$f":"GLASS_SPEC5(N41,O41,P41,Q41,R41,\"マスターシート!A3:F433\")","v":"none"},"○",null,"　","　","　",2.33,"計算/試験",0.79,{"$f":"VALUE_U_ETA_2(V41,X41,N41,S41,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},{"$f":"VALUE_U_ETA(X41,N41,S41,\"DATA BASE\",\"A\",\"F\",\"J3:J433\")","v":""},"計算/試験","日本サッシ","ＡＪドア"]
[23,"１階","キッチン","ＡＷ-19","北","ドア","勝手口ドア","06010",640,970,0.62080000000000002,"計算/試験","ドア",{"$f":"VLOOKUP(M42,'プルダウン項目 (2)'!M27:N42,2,0)","v":7},"複層","LowE（日射取得型）","A",15,"none","○",null,null,null,null,2.33,"計算/試験",0.79,"","","計算/試験","日本サッシ","ＡＪ勝手口ドア"]
[24,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,"　","　","　","　","　"]
[25,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,"　","　","　","　","　"]
[26,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,"　","　","　","　","　"]
[null,null,null,null,null,null,null,"合計開口面積",null,null,{"$f":"SUM(K18:K45)","v":29.797549999999987},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"一般社団法人　日本サッシ協会 標準書式　　2021.4.1"]
[]
[null,"≪注記≫ベージュ色のセル部分は、国立研究開発法人　建築研究所のホームページに掲載されている「住宅・住戸の外皮性能計算条件入力シート」へ、外皮性能を入力する際の必要項目を示す。"]
[null,"※１≪建具の仕様≫",null,null,null,"　１：（一重）木製または樹脂製",null,null,null,null,"　２：（一重）アルミ樹脂複合製",null,null,"３：（一重）金属製熱遮断構造　　",null,null,"３：（一重）金属製【アルミＰＧ・ＳＧ】",null,null,null,null,null,null,"５：（二重）金属製＋樹脂内窓"]
[null,null,null,null,null,"　６：（二重）　金属製＋金属製",null,null,null,null,"　７：ドア（框ドアを除く）",null,null,"８：引戸"]

{"sheet":"Ａシート　アルミPG 記入例","index":1,"n_rows":50,"n_cols":32,"rows_kept":50,"cut":false,"hidden":false,"merged":[[0,28,0,31],[1,29,1,31],[2,17,2,18],[2,19,2,24],[2,26,2,31],[3,23,4,27],[3,28,4,29],[3,30,4,31],[4,1,5,7],[5,8,8,9],[5,10,5,12],[5,13,6,18],[5,19,8,22],[5,23,8,27],[5,28,8,29],[3,1,3,5],[3,8,4,9],[3,10,3,12],[3,13,4,18],[3,19,4,22],[5,30,8,31],[6,1,6,5],[7,1,8,7],[7,10,7,12],[7,13,7,18],[8,10,8,12],[8,13,8,18],[9,8,9,9],[10,11,12,11],[10,12,11,12],[10,13,15,13],[10,14,11,17],[14,8,15,8],[14,9,15,9],[14,10,15,10],[10,30,15,30],[10,31,15,31],[11,1,15,1],[11,2,15,2],[11,3,15,3],[11,4,15,4],[11,5,15,5],[11,6,15,6],[10,18,15,18],[12,20,12,23],[12,24,13,25],[12,26,13,29],[13,11,15,11],[13,20,15,20],[13,21,15,21],[13,22,15,22],[14,26,15,26],[12,12,15,12],[12,14,15,14],[12,15,15,15],[12,16,15,16],[12,17,15,17],[12,19,15,19],[14,27,15,27],[14,28,15,28],[14,29,15,29],[16,1,16,2],[16,7,16,9],[16,14,16,17],[16,19,16,23],[16,26,16,28],[11,7,15,7],[11,8,11,10],[11,24,11,29],[12,8,13,10],[10,19,11,23],[10,24,10,29],[13,23,15,23],[14,25,15,25],[45,7,45,9],[45,26,45,31],[48,1,49,4],[38,1,38,31],[39,1,39,2],[39,7,39,9],[39,12,39,13],[39,14,39,18],[39,19,39,23],[39,26,39,28]]}
[]
[null,"外部開口部リスト２０２１年版 （兼 製品保証及び納入明細書）",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"記入例【アルミＰＧ】",null,null,null,null,null,null,null,null,null,null,null,"〔NO．　／　〕"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"現場納入日",null,"　　　　年　　月　　日",null,null,null,null,null,"取付確認日","　　　　年　　月　　日"]
[null,"物件の名称",null,null,null,null,null,null,"地域区分",null,"販売店名(代表者名）",null,null,"株式会社 〇〇サッシ販売",null,null,null,null,null,"取扱い事業所",null,null,null,"組立事業所登録NO.",null,null,null,null,"施工（管理）者　　　　　　　　　　　　　　　　　　　　　　",null,"納入確認者　　　　　　　　　　　　　　　　"]
[null,"〇△様邸 新築工事"]
[null,null,null,null,null,null,null,null,6,null,"取扱い事業所名",null,null,"株式会社 〇〇サッシ販売　△△営業所",null,null,null,null,null,"印",null,null,null,"１３－〇〇〇〇",null,null,null,null,"印",null,"印"]
[null,"物件の所在地 （又は地番）"]
[null,"〇〇県××市△△　〇丁目△番地×号",null,null,null,null,null,null,null,null,"事業所住所",null,null,"〇〇県△△市××　１２３－４"]
[null,null,null,null,null,null,null,null,null,null,"TEL",null,null,"０１２３-４５-６７８９"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"記入区分","建具　　　　　　　　　　　　　　仕様","　※１参照（サッシ協ＨＰ）","ガラス仕様 　厚さ・種類　　　　　　　　　　　　　　　　　〔①～④各項目を全て記入〕",null,null,null,"　※2参照（サッシ協ＨＰ）","付属部材",null,null,null,null,"住宅性能表示制度の必須項目",null,null,null,null,null,"　　サッシメーカー","　　シリーズ名又は記号"]
[null,"設置階","部位（部屋）","建具番号（窓番）","方位","窓・ドア区分","開閉形式","サイズ呼称","開口面積",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"温熱環境・エネルギー消費量"]
[null,null,null,null,null,null,null,null,"※外法寸法　　　　　　　　　　　　　　　　　　　　　（小数点第2位まで）",null,null,null,"種類",null,"①ガラス種類","②Ｌｏｗ－Ｅの有無","③中空層種類","④中空層厚み",null,"なし","あり",null,null,null,"熱貫流率\n　U値\n［W/㎡K］",null,"日射熱取得率  \nη値"]
[null,null,null,null,null,null,null,null,null,null,null,"仕様　　　　　　　　　　　　　　　　　　　　　　又は　　　　　　　計算　　　　　　　　　　（試験）",null,null,null,null,null,null,null,null,"シャッター・雨戸","和障子","風除室","外付ブラインド"]
[null,null,null,null,null,null,null,null,"外法　　 W　　　　（㎜）","外法　　　　　H　　　　　  （㎜）","W×H　　　（㎡）",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"性能根拠","付属\n部材\nなし","和障子","外付　　　　　　　　　　　　ブラインド","性能根拠"]
[]
[null,"選  択",null,"直接記入","選  択","選  択","選     択","直接記入",null,null,"自動表記","選  択","選     択","自動表記","選     択",null,null,null,"自動表記","選     択",null,null,null,null,"自動表記/直接入力","自動表記","自動表記/直接入力",null,null,"自動表記","選   択","直接記入"]
[1,"１階","リビング","ＡＷ-1","南","一重窓","引違い","16520",1690,2030,{"$f":"I18*J18/1000000","v":3.4306999999999999},"仕様","アルミＰＧ",{"$f":"VLOOKUP(M18,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,{"$f":"GLASS_SPEC5(N18,O18,P18,Q18,R18,\"マスターシート!A3:F433\")","v":95},"○","　","　","　","　",{"$f":"VALUE_U_ETA_P(N18,S18,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":4.07},{"$f":"VLOOKUP(L18,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},{"$f":"VALUE_U_ETA(T18,N18,S18,\"DATA BASE\",\"A\",\"F\",\"H3:H433\")","v":0.63},{"$f":"VALUE_U_ETA_2(V18,X18,N18,S18,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},{"$f":"VALUE_U_ETA(X18,N18,S18,\"DATA BASE\",\"A\",\"F\",\"J3:J433\")","v":""},{"$f":"VLOOKUP(L18,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[2,"１階","リビング","ＡＷ-2","南","一重窓","引違い","16520",1690,2030,{"$f":"I19*J19/1000000","v":3.4306999999999999},"仕様","アルミＰＧ",{"$f":"VLOOKUP(M19,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,{"$f":"GLASS_SPEC5(N19,O19,P19,Q19,R19,\"マスターシート!A3:F433\")","v":95},"○","　",null,null,null,{"$f":"VALUE_U_ETA_P(N19,S19,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":4.07},{"$f":"VLOOKUP(L19,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},{"$f":"VALUE_U_ETA(T19,N19,S19,\"DATA BASE\",\"A\",\"F\",\"H3:H433\")","v":0.63},{"$f":"VALUE_U_ETA_2(V19,X19,N19,S19,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},"",{"$f":"VLOOKUP(L19,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[3,"１階","和室","ＡＷ-3","南","一重窓","引違い","25620",2600,2030,5.2779999999999996,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M20,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　",null,null,null,{"$f":"VALUE_U_ETA_P(N20,S20,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":4.07},{"$f":"VLOOKUP(L20,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},{"$f":"VALUE_U_ETA(T20,N20,S20,\"DATA BASE\",\"A\",\"F\",\"H3:H433\")","v":0.63},{"$f":"VALUE_U_ETA_2(V20,X20,N20,S20,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},"",{"$f":"VLOOKUP(L20,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[4,"２階","寝室","ＡＷ-4","南","一重窓","引違い","16509",1690,970,1.6393,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M21,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"　","　","○","　",null,{"$f":"VALUE_U_ETA_P(N21,S21,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":4.07},{"$f":"VLOOKUP(L21,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"",0.3,"",{"$f":"VLOOKUP(L21,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[5,"２階","子供室","ＡＷ-5","南","一重窓","引違い","16520",1690,2030,3.4306999999999999,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M22,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　",null,"　","　",{"$f":"VALUE_U_ETA_P(N22,S22,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":4.07},{"$f":"VLOOKUP(L22,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L22,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[6,"２階","子供室","ＡＷ-6","南","一重窓","引違い","16520",1690,2030,3.4306999999999999,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M23,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L23,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L23,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[7,"１階","トイレ","ＡＷ-7","北","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M24,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L24,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L24,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[8,"１階","洗面所","ＡＷ-8","北","一重窓","たてすべり出し","06009",640,970,0.62080000000000002,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M25,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L25,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L25,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[9,"１階","ホール","ＡＷ-9","北","一重窓","ＦＩＸ","02611",300,1170,0.35099999999999998,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M26,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L26,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L26,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[10,"２階","ホール","ＡＷ-10","北","一重窓","ＦＩＸ","02609",300,970,0.29099999999999998,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M27,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L27,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L27,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[11,"１階","トイレ","ＡＷ-11","北","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M28,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",15,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L28,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L28,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[12,"１階","リビング","ＡＷ-12","東","一重窓","引違い","16511",1690,1170,1.9773000000000001,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M29,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L29,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L29,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[13,"１階","キッチン","ＡＷ-13","東","一重窓","引違い","11907",1235,770,0.95094999999999996,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M30,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",15,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L30,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L30,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[14,"２階","子供室","ＡＷ-14","東","一重窓","たてすべり出し","06009",640,970,0.62080000000000002,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M31,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L31,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L31,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[15,"１階","浴室","ＡＷ-15","西","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M32,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",15,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L32,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L32,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[16,"２階","寝室","ＡＷ-16","西","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M33,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",15,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L33,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L33,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[17,"２階","クローゼット","ＡＷ-17","西","一重窓","たてすべり出し","06009",640,970,0.62080000000000002,"仕様","アルミＰＧ",{"$f":"VLOOKUP(M34,'プルダウン項目 (2)'!M27:N42,2,0)","v":3},"複層","無し","A",16,95,"○","　","　","　","　",4.07,{"$f":"VLOOKUP(L34,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.63,"","",{"$f":"VLOOKUP(L34,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","ＰＧサッシ"]
[]
[]
[]
[]
[null,"◎以下の行は直接入力です。"]
[null,"選  択",null,"直接記入","選  択","選  択","選   択","直接記入",null,null,"自動表記","直接記入","直接記入",null,"直接記入",null,null,null,null,"選   択",null,null,null,null,"直接記入","直接記入","直接記入",null,null,"直接記入","選  択","直接記入"]
[22,"１階","玄関","ＡＷ-18","西","ドア","玄関ドア","06009",640,970,{"$f":"I41*J41/1000000","v":0.62080000000000002},"計算/試験","ドア",{"$f":"VLOOKUP(M41,'プルダウン項目 (2)'!M27:N42,2,0)","v":7},"ガラス無し","無し","N","無し",{"$f":"GLASS_SPEC5(N41,O41,P41,Q41,R41,\"マスターシート!A3:F433\")","v":"none"},"○","　","　","　","　",3.49,"計算/試験",0.11899999999999999,{"$f":"VALUE_U_ETA_2(V41,X41,N41,S41,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},{"$f":"VALUE_U_ETA(X41,N41,S41,\"DATA BASE\",\"A\",\"F\",\"J3:J433\")","v":""},"計算/試験","日本サッシ","ＰＧ引戸"]
[23,"１階","キッチン","ＡＷ-19","北","ドア","勝手口ドア","06010",640,970,0.62080000000000002,"計算/試験","ドア",{"$f":"VLOOKUP(M42,'プルダウン項目 (2)'!M27:N42,2,0)","v":7},"複層","無し","A",15,"none","○",null,null,null,null,4.07,"計算/試験",0.13800000000000001,"","","計算/試験","日本サッシ","ＰＧ勝手口ドア"]
[24,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,"　","　","　","　","　"]
[25,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,"　","　","　","　","　"]
[26,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,"　","　","　","　","　"]
[null,null,null,null,null,null,null,"合計開口面積",null,null,{"$f":"SUM(K18:K45)","v":29.797549999999987},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"一般社団法人　日本サッシ協会 標準書式　　2021.4.1"]
[]
[null,"≪注記≫ベージュ色のセル部分は、国立研究開発法人　建築研究所のホームページに掲載されている「住宅・住戸の外皮性能計算条件入力シート」へ、外皮性能を入力する際の必要項目を示す。"]
[null,"※１≪建具の仕様≫",null,null,null,"　１：（一重）木製または樹脂製",null,null,null,null,"　２：（一重）アルミ樹脂複合製",null,null,"３：（一重）金属製熱遮断構造　　",null,null,"３：（一重）金属製【アルミＰＧ・ＳＧ】",null,null,null,null,null,null,"５：（二重）金属製＋樹脂内窓"]
[null,null,null,null,null,"　６：（二重）　金属製＋金属製",null,null,null,null,"　７：ドア（框ドアを除く）",null,null,"８：引戸"]

{"sheet":"Ａシート　樹脂 記入例","index":2,"n_rows":50,"n_cols":32,"rows_kept":50,"cut":false,"hidden":false,"merged":[[48,1,49,4],[45,26,45,31],[3,28,4,29],[3,30,4,31],[5,28,8,29],[5,30,8,31],[10,19,11,23],[10,30,15,30],[12,19,15,19],[10,31,15,31],[3,1,3,5],[3,8,4,9],[3,10,3,12],[3,13,4,18],[3,19,4,22],[4,1,5,7],[0,28,0,31],[1,29,1,31],[2,17,2,18],[2,19,2,24],[2,26,2,31],[5,8,8,9],[5,10,5,12],[5,13,6,18],[5,19,8,22],[6,1,6,5],[7,1,8,7],[7,10,7,12],[7,13,7,18],[8,10,8,12],[8,13,8,18],[9,8,9,9],[10,11,12,11],[10,12,11,12],[10,13,15,13],[11,8,11,10],[14,8,15,8],[14,9,15,9],[14,10,15,10],[12,8,13,10],[12,12,15,12],[45,7,45,9],[10,14,11,17],[10,18,15,18],[12,14,15,14],[12,15,15,15],[12,16,15,16],[12,17,15,17],[11,7,15,7],[39,14,39,18],[39,12,39,13],[13,11,15,11],[5,23,8,27],[3,23,4,27],[10,24,10,29],[11,24,11,29],[12,24,13,25],[12,26,13,29],[12,20,12,23],[13,20,15,20],[13,21,15,21],[13,22,15,22],[13,23,15,23],[14,26,15,26],[14,27,15,27],[14,28,15,28],[14,25,15,25],[14,29,15,29],[16,19,16,23],[39,7,39,9],[39,19,39,23],[38,1,38,31],[39,26,39,28],[16,26,16,28],[16,1,16,2],[11,1,15,1],[11,2,15,2],[39,1,39,2],[16,7,16,9],[16,14,16,17],[11,3,15,3],[11,4,15,4],[11,5,15,5],[11,6,15,6]]}
[]
[null,"外部開口部リスト２０２１年版 （兼 製品保証及び納入明細書）",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"記入例【樹脂】",null,null,null,null,null,null,null,null,null,null,null,"〔NO．　／　〕"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"現場納入日",null,"　　　　年　　月　　日",null,null,null,null,null,"取付確認日","　　　　年　　月　　日"]
[null,"物件の名称",null,null,null,null,null,null,"地域区分",null,"販売店名(代表者名）",null,null,"株式会社 〇〇サッシ販売",null,null,null,null,null,"取扱い事業所",null,null,null,"組立事業所登録NO.",null,null,null,null,"施工（管理）者　　　　　　　　　　　　　　　　　　　　　　",null,"納入確認者　　　　　　　　　　　　　　　　"]
[null,"〇△様邸 新築工事"]
[null,null,null,null,null,null,null,null,6,null,"取扱い事業所名",null,null,"株式会社 〇〇サッシ販売　△△営業所",null,null,null,null,null,"印",null,null,null,"１３－〇〇〇〇",null,null,null,null,"印",null,"印"]
[null,"物件の所在地 （又は地番）"]
[null,"〇〇県××市△△　〇丁目△番地×号",null,null,null,null,null,null,null,null,"事業所住所",null,null,"〇〇県△△市××　１２３－４"]
[null,null,null,null,null,null,null,null,null,null,"TEL",null,null,"０１２３-４５-６７８９"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"記入区分","建具　　　　　　　　　　　　　　仕様","　※１参照（サッシ協ＨＰ）","ガラス仕様 　厚さ・種類　　　　　　　　　　　　　　　　　〔①～④各項目を全て記入〕",null,null,null,"　※2参照（サッシ協ＨＰ）","付属部材",null,null,null,null,"住宅性能表示制度の必須項目",null,null,null,null,null,"　　サッシメーカー","　　シリーズ名又は記号"]
[null,"設置階","部位（部屋）","建具番号（窓番）","方位","窓・ドア区分","開閉形式","サイズ呼称","開口面積",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"温熱環境・エネルギー消費量"]
[null,null,null,null,null,null,null,null,"※外法寸法　　　　　　　　　　　　　　　　　　　　　（小数点第2位まで）",null,null,null,"種類",null,"①ガラス種類","②Ｌｏｗ－Ｅの有無","③中空層種類","④中空層厚み",null,"なし","あり",null,null,null,"熱貫流率\n　U値\n［W/㎡K］",null,"日射熱取得率  \nη値"]
[null,null,null,null,null,null,null,null,null,null,null,"仕様　　　　　　　　　　　　　　　　　　　　　　又は　　　　　　　計算　　　　　　　　　　（試験）",null,null,null,null,null,null,null,null,"シャッター・雨戸","和障子","風除室","外付ブラインド"]
[null,null,null,null,null,null,null,null,"外法　　 W　　　　（㎜）","外法　　　　　H　　　　　  （㎜）","W×H　　　（㎡）",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"性能根拠","付属\n部材\nなし","和障子","外付　　　　　　　　　　　　ブラインド","性能根拠"]
[]
[null,"選  択",null,"直接記入","選  択","選  択","選     択","直接記入",null,null,"自動表記","選  択","選     択","自動表記","選     択",null,null,null,"自動表記","選     択",null,null,null,null,"自動表記/直接入力","自動表記","自動表記/直接入力",null,null,"自動表記","選   択","直接記入"]
[1,"１階","リビング","ＡＷ-1","南","一重窓","引違い","16520",1690,2030,{"$f":"I18*J18/1000000","v":3.4306999999999999},"仕様","樹脂",{"$f":"VLOOKUP(M18,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,{"$f":"GLASS_SPEC5(N18,O18,P18,Q18,R18,\"マスターシート!A3:F433\")","v":31},"○","　","　","　","　",{"$f":"VALUE_U_ETA_P(N18,S18,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.15},{"$f":"VLOOKUP(L18,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},{"$f":"VALUE_U_ETA(T18,N18,S18,\"DATA BASE\",\"A\",\"F\",\"H3:H433\")","v":0.46},{"$f":"VALUE_U_ETA_2(V18,X18,N18,S18,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},{"$f":"VALUE_U_ETA(X18,N18,S18,\"DATA BASE\",\"A\",\"F\",\"J3:J433\")","v":""},{"$f":"VLOOKUP(L18,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[2,"１階","リビング","ＡＷ-2","南","一重窓","引違い","16520",1690,2030,{"$f":"I19*J19/1000000","v":3.4306999999999999},"仕様","樹脂",{"$f":"VLOOKUP(M19,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,{"$f":"GLASS_SPEC5(N19,O19,P19,Q19,R19,\"マスターシート!A3:F433\")","v":31},"○","　",null,null,null,{"$f":"VALUE_U_ETA_P(N19,S19,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.15},{"$f":"VLOOKUP(L19,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},{"$f":"VALUE_U_ETA(T19,N19,S19,\"DATA BASE\",\"A\",\"F\",\"H3:H433\")","v":0.46},{"$f":"VALUE_U_ETA_2(V19,X19,N19,S19,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},"",{"$f":"VLOOKUP(L19,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[3,"１階","和室","ＡＷ-3","南","一重窓","引違い","25620",2600,2030,5.2779999999999996,"仕様","樹脂",{"$f":"VLOOKUP(M20,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　",null,null,null,{"$f":"VALUE_U_ETA_P(N20,S20,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.15},{"$f":"VLOOKUP(L20,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},{"$f":"VALUE_U_ETA(T20,N20,S20,\"DATA BASE\",\"A\",\"F\",\"H3:H433\")","v":0.46},{"$f":"VALUE_U_ETA_2(V20,X20,N20,S20,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},"",{"$f":"VLOOKUP(L20,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[4,"２階","寝室","ＡＷ-4","南","一重窓","引違い","16509",1690,970,1.6393,"仕様","樹脂",{"$f":"VLOOKUP(M21,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"　","　","○","　",null,{"$f":"VALUE_U_ETA_P(N21,S21,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.15},{"$f":"VLOOKUP(L21,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"",0.27,"",{"$f":"VLOOKUP(L21,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[5,"２階","子供室","ＡＷ-5","南","一重窓","引違い","16520",1690,2030,3.4306999999999999,"仕様","樹脂",{"$f":"VLOOKUP(M22,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　",null,"　","　",{"$f":"VALUE_U_ETA_P(N22,S22,\"DATA BASE\",\"A\",\"F\",\"G3:G433\")","v":2.15},{"$f":"VLOOKUP(L22,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L22,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[6,"２階","子供室","ＡＷ-6","南","一重窓","引違い","16520",1690,2030,3.4306999999999999,"仕様","樹脂",{"$f":"VLOOKUP(M23,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L23,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L23,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[7,"１階","トイレ","ＡＷ-7","北","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","樹脂",{"$f":"VLOOKUP(M24,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L24,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L24,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[8,"１階","洗面所","ＡＷ-8","北","一重窓","たてすべり出し","06009",640,970,0.62080000000000002,"仕様","樹脂",{"$f":"VLOOKUP(M25,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L25,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L25,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[9,"１階","ホール","ＡＷ-9","北","一重窓","ＦＩＸ","02611",300,1170,0.35099999999999998,"仕様","樹脂",{"$f":"VLOOKUP(M26,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L26,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L26,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[10,"２階","ホール","ＡＷ-10","北","一重窓","ＦＩＸ","02609",300,970,0.29099999999999998,"仕様","樹脂",{"$f":"VLOOKUP(M27,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L27,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L27,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[11,"１階","トイレ","ＡＷ-11","北","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","樹脂",{"$f":"VLOOKUP(M28,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",15,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L28,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L28,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[12,"１階","リビング","ＡＷ-12","東","一重窓","引違い","16511",1690,1170,1.9773000000000001,"仕様","樹脂",{"$f":"VLOOKUP(M29,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L29,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L29,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[13,"１階","キッチン","ＡＷ-13","東","一重窓","引違い","11907",1235,770,0.95094999999999996,"仕様","樹脂",{"$f":"VLOOKUP(M30,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",15,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L30,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L30,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[14,"２階","子供室","ＡＷ-14","東","一重窓","たてすべり出し","06009",640,970,0.62080000000000002,"仕様","樹脂",{"$f":"VLOOKUP(M31,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L31,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L31,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[15,"１階","浴室","ＡＷ-15","西","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","樹脂",{"$f":"VLOOKUP(M32,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",15,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L32,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L32,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[16,"２階","寝室","ＡＷ-16","西","一重窓","上げ下げ","06009",640,970,0.62080000000000002,"仕様","樹脂",{"$f":"VLOOKUP(M33,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",15,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L33,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L33,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[17,"２階","クローゼット","ＡＷ-17","西","一重窓","たてすべり出し","06009",640,970,0.62080000000000002,"仕様","樹脂",{"$f":"VLOOKUP(M34,'プルダウン項目 (2)'!M27:N42,2,0)","v":1},"複層","LowE（日射取得型）","G",16,31,"○","　","　","　","　",2.15,{"$f":"VLOOKUP(L34,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},0.46,"","",{"$f":"VLOOKUP(L34,'プルダウン項目 (2)'!N6:O8,2,0)","v":"ｻｯｼ協ＨＰ"},"日本サッシ","Ｊサッシ"]
[]
[]
[]
[]
[null,"◎以下の行は直接入力です。"]
[null,"選  択",null,"直接記入","選  択","選  択","選   択","直接記入",null,null,"自動表記","直接記入","直接記入",null,"直接記入",null,null,null,null,"選   択",null,null,null,null,"直接記入","直接記入","直接記入",null,null,"直接記入","選  択","直接記入"]
[22,"１階","玄関","ＡＷ-18","西","ドア","玄関ドア","06009",640,970,{"$f":"I41*J41/1000000","v":0.62080000000000002},"計算/試験","ドア",{"$f":"VLOOKUP(M41,'プルダウン項目 (2)'!M27:N42,2,0)","v":7},"ガラス無し","無し","N","無し",{"$f":"GLASS_SPEC5(N41,O41,P41,Q41,R41,\"マスターシート!A3:F433\")","v":"none"},"○",null,"　","　","　",2.33,"計算/試験",0.79,{"$f":"VALUE_U_ETA_2(V41,X41,N41,S41,\"DATA BASE\",\"A\",\"F\",\"I3:I433\")","v":""},{"$f":"VALUE_U_ETA(X41,N41,S41,\"DATA BASE\",\"A\",\"F\",\"J3:J433\")","v":""},"計算/試験","日本サッシ","Ｊドア"]
[23,"１階","キッチン","ＡＷ-19","北","ドア","勝手口ドア","06010",640,970,0.62080000000000002,"計算/試験","ドア",{"$f":"VLOOKUP(M42,'プルダウン項目 (2)'!M27:N42,2,0)","v":7},"複層","LowE（日射取得型）","G",15,"none","○",null,null,null,null,2.33,"計算/試験",0.79,"","","計算/試験","日本サッシ","Ｊ勝手口ドア"]
[24,null,null,null,null,null,null,null,null,null,{"$f":"I43*J43/1000000","v":0},null,null,null,null,null,null,null,null,"　","　","　","　","　"]
[25,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,"　","　","　","　","　"]
[26,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,"　","　","　","　","　"]
[null,null,null,null,null,null,null,"合計開口面積",null,null,{"$f":"SUM(K18:K45)","v":29.797549999999987},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"一般社団法人　日本サッシ協会 標準書式　　2021.4.1"]
[]
[null,"≪注記≫ベージュ色のセル部分は、国立研究開発法人　建築研究所のホームページに掲載されている「住宅・住戸の外皮性能計算条件入力シート」へ、外皮性能を入力する際の必要項目を示す。"]
[null,"※１≪建具の仕様≫",null,null,null,"　１：（一重）木製または樹脂製",null,null,null,null,"　２：（一重）アルミ樹脂複合製",null,null,"３：（一重）金属製熱遮断構造　　",null,null,"３：（一重）金属製【アルミＰＧ・ＳＧ】",null,null,null,null,null,null,"５：（二重）金属製＋樹脂内窓"]
[null,null,null,null,null,"　６：（二重）　金属製＋金属製",null,null,null,null,"　７：ドア（框ドアを除く）",null,null,"８：引戸"]

{"sheet":"プルダウン項目 (2)","index":3,"n_rows":243,"n_cols":15,"rows_kept":243,"cut":false,"hidden":true,"merged":[[3,2,3,3],[3,10,3,11],[65,1,65,2],[83,7,83,8],[0,10,0,11]]}
[null,"７）書式のプルダウン項目",null,null,null,null,null,null,null,null,"2021.04.1"]
[null,"　　下記項目は、プルダウンにより選択することができます。"]
[]
[null,"９．設置階","１０．部位（部屋）",null,"１２．方位","１３．窓・ドア区分","１４．開閉形式",null,null,null,"１７．仕様又は計算、試験"]
[null,"１階","玄関",null,"南","一重窓","引違い",null,null,null,"仕様",null,null,"28　30"]
[null,"２階","和室",null,"南西","二重窓","ＦＩＸ",null,null,null,"計算/試験",null,null,"仕様","ｻｯｼ協ＨＰ"]
[null,"３階","寝室",null,"南東","ドア","上げ下げ",null,null,null,null,null,null,"計算/試験","計算/試験"]
[null,"地下","子供室",null,"西","引戸","たてすべり出し",null,null,null,null,null,null,"-","-"]
[null,null,"洋間",null,"東",null,"すべり出し"]
[null,null,"トイレ",null,"北西",null,"外倒し"]
[null,null,"洗面所",null,"北東",null,"内倒し"]
[null,null,"浴室",null,"北",null,"ルーバー"]
[null,null,"キッチン",null,"屋根上面",null,"オーニング"]
[null,null,"リビング",null,"下面",null,"突き出し"]
[null,null,"ダイニング",null,null,null,"出窓"]
[null,null,"ＬＤK",null,null,null,"天窓"]
[null,null,"ホール",null,null,null,"折りたたみ",null,null,"１１．建具番号は事業所が入力"]
[null,null,"クローゼット",null,null,null,"ガラスブロック"]
[null,null,"廊下",null,null,null,"その他窓",null,null,"１５．サイズ呼称は事業所が入力"]
[null,null,"階段",null,null,null,"玄関ドア",null,null,"１６．外法寸法（ｍｍ）は事業所が入力"]
[null,null,"書斎",null,null,null,"玄関引戸",null,null,"１７．開口面積（㎡）は自動計算"]
[null,null,"縁側",null,null,null,"勝手口ドア"]
[null,null,"脱衣室",null,null,null,"勝手口引戸"]
[null,null,"地下室",null,null,null,"テラスドア"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"１９．建具仕様","ｻｯｼ協ＨＰ"]
[null,null,null,null,null,null,null,null,null,null,null,null,"樹脂",1]
[null,null,null,null,null,null,null,null,null,null,null,null,"アルミ樹脂複合",2]
[null,null,null,null,null,null,null,null,null,null,null,null,"アルミ熱遮断構造",3]
[null,null,null,null,null,null,null,null,null,null,null,null,"アルミＰＧ",3]
[null,null,null,null,null,null,null,null,null,null,null,null,"アルミＳＧ",3]
[null,null,null,null,null,null,null,null,null,null,null,null,"アルミＳＧ＋樹脂内窓",5]
[null,null,null,null,null,null,null,null,null,null,null,null,"木製",1]
[null,null,null,null,null,null,null,null,null,null,null,null,"アルミ木複合",2]
[null,null,null,null,null,null,null,null,null,null,null,null,"金属製＋金属製",6]
[null,null,null,null,null,null,null,null,null,null,null,null,"ドア",7]
[null,null,null,null,null,null,null,null,null,null,null,null,"引戸",8]
[]
[null,"赤字は、２０２１年４月１日に改訂。"]
[null,"１９．※１参照（ｻｯｼ協ＨＰ）は自動表記"]
[null,"【窓等の大部分がガラスで構成される開口部（一重構造の建具）の熱貫流率】"]
[null,1,"（一重）木製又は樹脂製　　"]
[null,2,"（一重）アルミ樹脂複合構造製　　"]
[null,3,"（一重）金属製熱遮断構造製"]
[null,3,"（一重）金属製【アルミPG・SG】"]
[null,5,"（二重）金属製＋樹脂内窓"]
[null,"【ドア等の大部分がガラスで構成されない開口部】・・・熱貫流率は自動表記されません。直接入力してください。"]
[null,7,"ドア１：金属製熱遮断構造の枠＋金属製高断熱フラッシュ構造の戸"]
[null,7,"ドア２：金属製熱遮断構造の枠＋金属製断熱フラッシュ構造の戸"]
[null,7,"ドア３：金属製熱遮断構造の枠＋金属製フラッシュ構造の戸"]
[null,7,"ドア４：金属製熱遮断構造の枠＋金属製ハニカムフラッシュ構造の戸","戸：金属製断熱フラッシュ構造"]
[null,7,"ドア５：複合材料製の枠＋金属製高断熱フラッシュ構造の戸"]
[null,7,"ドア６：複合材料製の枠＋金属製断熱フラッシュ構造の戸"]
[null,7,"ドア７：複合材料製の枠＋金属製フラッシュ構造の戸"]
[null,7,"ドア８：複合材料製の枠＋金属製ハニカムフラッシュ構造の戸"]
[null,7,"ドア９：金属製またはその他の枠＋金属製フラッシュ構造の戸"]
[null,7,"ドア１０：金属製またはその他の枠＋金属製ハニカムフラッシュ構造の戸"]
[null,7,"ドア１１：金属製またはその他の枠＋金属製またはその他の構造の戸"]
[]
[]
[]
[]
[]
[]
[]
[null,"２１．①ガラス種類",null,"２２．②Ｌｏｗ－Ｅの有無",null,null,null,"２３．④中空層種類",null,"２４．⑤中空層厚み"]
[null,null,"三層",null,"ダブルLowE（日射取得型）",null,null,"G","ガス",null,"16×2"]
[null,null,"複層",null,"ダブルLowE（日射遮蔽型）",null,null,"A","空気",null,"15×2"]
[null,null,"単板",null,"LowE（日射取得型）",null,null,"N","無し",null,"14×2"]
[null,null,"単板+複層",null,"LowE（日射遮蔽型）",null,null,null,null,null,"13×2"]
[null,null,"単板+単板",null,"LowE",null,null,null,null,null,"12×2"]
[null,null,"ガラス無し",null,"単板",null,null,null,null,null,"11×2"]
[null,null,null,null,"無し",null,null,null,null,null,"10×2"]
[null,null,null,null,null,null,null,null,null,null,"9×2"]
[null,null,null,null,null,null,null,null,null,null,"8×2"]
[null,null,null,null,null,null,null,null,null,null,"7×2"]
[null,null,null,null,null,null,null,null,null,null,"6×2"]
[null,null,null,null,null,null,null,null,null,null,16]
[null,null,null,null,null,null,null,null,null,null,15]
[null,null,null,null,null,null,null,null,null,null,14]
[null,null,null,null,null,null,null,null,null,null,13]
[null,null,null,null,null,null,null,null,null,null,12]
[null,null,null,null,null,null,null,null,null,null,11]
[null,null,null,null,null,null,null,null,null,null,10]
[null,null,null,null,null,null,null,null,null,null,9]
[null,null,null,null,null,null,null,null,null,null,8]
[null,null,null,null,null,null,null,null,null,null,7]
[null,null,null,null,null,null,null,null,null,null,6]
[null,null,null,null,null,null,null,null,null,null,5]
[null,null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,null,null,null,"単板"]
[null,null,null,null,null,null,null,null,null,null,"無し"]
[]
[null,"２５．※２参照は自動表記"]
[null,null,"窓の熱貫流率のガラスの仕様"]
[null,1,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ１３以上×２）日射取得型",null,null,null,null,null,null,"Ｐ．７１、７２　差替"]
[null,2,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ１３以上×２）日射遮蔽型"]
[null,3,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ１０以上G１３未満×２）日射取得型"]
[null,4,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ１０以上G１３未満×２）日射遮蔽型"]
[null,5,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ７以上G１０未満×２）日射取得型"]
[null,6,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ７以上G１０未満×２）日射遮蔽型"]
[null,7,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ７未満×２）日射取得型"]
[null,8,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ７未満×２）日射遮蔽型"]
[null,9,"ダブルＬｏｗ-Ｅ　三層複層（Ａ１３以上×２）日射取得型"]
[null,10,"ダブルＬｏｗ-Ｅ　三層複層（Ａ１３以上×２）日射遮蔽型"]
[null,11,"ダブルＬｏｗ-Ｅ　三層複層（Ａ９以上A１３未満×２）日射取得型"]
[null,12,"ダブルＬｏｗ-Ｅ　三層複層（Ａ９以上A１３未満×２）日射遮蔽型"]
[null,13,"ダブルＬｏｗ-Ｅ　三層複層（Ａ７以上A９未満×２）日射取得型"]
[null,14,"ダブルＬｏｗ-Ｅ　三層複層（Ａ７以上A９未満×２）日射遮蔽型"]
[null,15,"ダブルＬｏｗ-Ｅ　三層複層（Ａ７未満×２）日射取得型"]
[null,16,"ダブルＬｏｗ-Ｅ　三層複層（Ａ７未満×２）日射遮蔽型"]
[null,17,"Ｌｏｗ-Ｅ　三層複層（Ｇ１０以上×２）日射取得型"]
[null,18,"Ｌｏｗ-Ｅ　三層複層（Ｇ１０以上×２）日射遮蔽型"]
[null,19,"Ｌｏｗ-Ｅ　三層複層（Ｇ１０未満×２）日射取得型"]
[null,20,"Ｌｏｗ-Ｅ　三層複層（Ｇ１０未満×２）日射遮蔽型"]
[null,21,"Ｌｏｗ-Ｅ　三層複層（Ａ１３以上×２）日射取得型"]
[null,22,"Ｌｏｗ-Ｅ　三層複層（Ａ１３以上×２）日射遮蔽型"]
[null,23,"Ｌｏｗ-Ｅ　三層複層（Ａ９以上A１３未満×２）日射取得型"]
[null,24,"Ｌｏｗ-Ｅ　三層複層（Ａ９以上A１３未満×２）日射遮蔽型"]
[null,25,"Ｌｏｗ-Ｅ　三層複層（Ａ７以上A９未満×２）日射取得型"]
[null,26,"Ｌｏｗ-Ｅ　三層複層（Ａ７以上A９未満×２）日射遮蔽型"]
[null,27,"Ｌｏｗ-Ｅ　三層複層（Ａ７未満×２）日射取得型"]
[null,28,"Ｌｏｗ-Ｅ　三層複層（Ａ７未満×２）日射遮蔽型"]
[null,29,"三層複層（Ａ1２以上×２）"]
[null,30,"三層複層（Ａ1２未満×２）"]
[null,31,"Ｌｏｗ-Ｅ　複層（Ｇ１０以上）日射取得型"]
[null,32,"Ｌｏｗ-Ｅ　複層（Ｇ１０以上）日射遮蔽型"]
[null,33,"Ｌｏｗ-Ｅ　複層（Ｇ８以上Ｇ１０未満）日射取得型"]
[null,34,"Ｌｏｗ-Ｅ　複層（Ｇ８以上Ｇ１０未満）日射遮蔽型"]
[null,35,"Ｌｏｗ-Ｅ　複層（Ｇ８未満）日射取得型"]
[null,36,"Ｌｏｗ-Ｅ　複層（Ｇ８未満）日射遮蔽型"]
[null,37,"Ｌｏｗ-Ｅ　複層（Ａ１４以上）日射取得型"]
[null,38,"Ｌｏｗ-Ｅ　複層（Ａ１４以上）日射遮蔽型"]
[null,39,"Ｌｏｗ-Ｅ　複層（Ａ１１以上Ａ１４未満）日射取得型"]
[null,40,"Ｌｏｗ-Ｅ　複層（Ａ１１以上Ａ１４未満）日射遮蔽型"]
[null,41,"Ｌｏｗ-Ｅ　複層（Ａ１１未満）日射取得型"]
[null,42,"Ｌｏｗ-Ｅ　複層（Ａ１１未満）日射遮蔽型"]
[null,43,"複層（Ａ１３以上）"]
[null,44,"複層（Ａ１３未満）"]
[null,45,"単板"]
[null,46,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ１２以上×２）日射取得型"]
[null,47,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ１２以上×２）日射遮蔽型"]
[null,48,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ８以上G１２未満×２）日射取得型"]
[null,49,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ８以上G１２未満×２）日射遮蔽型"]
[null,50,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ８未満×２）日射取得型"]
[null,51,"ダブルＬｏｗ-Ｅ　三層複層（Ｇ８未満×２）日射遮蔽型"]
[null,52,"ダブルＬｏｗ-Ｅ　三層複層（Ａ１６以上×２）日射取得型"]
[null,53,"ダブルＬｏｗ-Ｅ　三層複層（Ａ１６以上×２）日射遮蔽型"]
[null,54,"ダブルＬｏｗ-Ｅ　三層複層（Ａ１０以上A１６未満×２）日射取得型"]
[null,55,"ダブルＬｏｗ-Ｅ　三層複層（Ａ１０以上A１６未満×２）日射遮蔽型"]
[null,56,"ダブルＬｏｗ-Ｅ　三層複層（Ａ８以上A１０未満×２）日射取得型"]
[null,57,"ダブルＬｏｗ-Ｅ　三層複層（Ａ８以上A１０未満×２）日射遮蔽型"]
[null,58,"ダブルＬｏｗ-Ｅ　三層複層（Ａ８未満×２）日射取得型"]
[null,59,"ダブルＬｏｗ-Ｅ　三層複層（Ａ８未満×２）日射遮蔽型"]
[null,60,"Ｌｏｗ-Ｅ　三層複層（Ｇ１２以上×２）日射取得型"]
[null,61,"Ｌｏｗ-Ｅ　三層複層（Ｇ１２以上×２）日射遮蔽型"]
[null,62,"Ｌｏｗ-Ｅ　三層複層（Ｇ９以上Ｇ１２未満×２）日射取得型"]
[null,63,"Ｌｏｗ-Ｅ　三層複層（Ｇ９以上Ｇ１２未満×２）日射遮蔽型"]
[null,64,"Ｌｏｗ-Ｅ　三層複層（Ｇ９未満×２）日射取得型"]
[null,65,"Ｌｏｗ-Ｅ　三層複層（Ｇ９未満×２）日射遮蔽型"]
[null,66,"Ｌｏｗ-Ｅ　三層複層（Ａ１６以上×２）日射取得型"]
[null,67,"Ｌｏｗ-Ｅ　三層複層（Ａ１６以上×２）日射遮蔽型"]
[null,68,"Ｌｏｗ-Ｅ　三層複層（Ａ１２以上A１６未満×２）日射取得型"]
[null,69,"Ｌｏｗ-Ｅ　三層複層（Ａ１２以上A１６未満×２）日射遮蔽型"]
[null,70,"Ｌｏｗ-Ｅ　三層複層（Ａ１２未満×２）日射取得型"]
[null,71,"Ｌｏｗ-Ｅ　三層複層（Ａ１２未満×２）日射遮蔽型"]
[null,72,"三層複層（Ａ７以上×２）"]
[null,73,"三層複層（Ａ７未満×２）"]
[null,74,"Ｌｏｗ-Ｅ　複層（Ｇ１４以上）日射取得型"]
[null,75,"Ｌｏｗ-Ｅ　複層（Ｇ１４以上）日射遮蔽型"]
[null,76,"Ｌｏｗ-Ｅ　複層（Ｇ１４未満）日射取得型"]
[null,77,"Ｌｏｗ-Ｅ　複層（Ｇ１４未満）日射遮蔽型"]
[null,78,"Ｌｏｗ-Ｅ　複層（Ａ９以上）日射取得型"]
[null,79,"Ｌｏｗ-Ｅ　複層（Ａ９以上）日射遮蔽型"]
[null,80,"Ｌｏｗ-Ｅ　複層（Ａ９未満）日射取得型"]
[null,81,"Ｌｏｗ-Ｅ　複層（Ａ９未満）日射遮蔽型"]
[null,82,"複層（Ａ１１以上）"]
[null,83,"複層（Ａ１１未満）"]
[null,84,"単板"]
[null,85,"Ｌｏｗ-Ｅ　複層（Ｇ１０以上）日射取得型"]
[null,86,"Ｌｏｗ-Ｅ　複層（Ｇ１０以上）日射遮蔽型"]
[null,87,"Ｌｏｗ-Ｅ　複層（Ｇ１０未満）日射取得型"]
[null,88,"Ｌｏｗ-Ｅ　複層（Ｇ１０未満）日射遮蔽型"]
[null,89,"Ｌｏｗ-Ｅ　複層（Ａ１４以上）日射取得型"]
[null,90,"Ｌｏｗ-Ｅ　複層（Ａ１４以上）日射遮蔽型"]
[null,91,"Ｌｏｗ-Ｅ　複層（Ａ７以上Ａ１４未満）日射取得型"]
[null,92,"Ｌｏｗ-Ｅ　複層（Ａ７以上Ａ１４未満）日射遮蔽型"]
[null,93,"Ｌｏｗ-Ｅ　複層（Ａ７未満）日射取得型"]
[null,94,"Ｌｏｗ-Ｅ　複層（Ａ７未満）日射遮蔽型"]
[null,95,"複層（Ａ８以上）"]
[null,96,"複層（Ａ８未満）"]
[null,97,"単板"]
[null,null,"ドア・引戸の熱貫流率の建具の仕様（大部分がガラスで構成されないドア等） "]
[null,null,"＊自動計算しないので2021年改訂時より削除した。"]
[null,39,"Ｌｏｗ－Ｅ　複層（Ａ１０以上）又は「ガラスなし」"]
[null,40,"三層複層（Ａ１２以上×２）"]
[null,41,"複層（Ａ１０以上）"]
[null,42,"Ｌｏｗ－Ｅ　複層（Ａ６以上Ａ１０未満）"]
[null,43,"Ｌｏｗ－Ｅ　複層（Ｇ１２以上）又は「ガラスなし」"]
[null,44,"複層（Ａ１２以上）又は「ガラスなし」"]
[null,45,"複層（Ａ４以上）又は「ガラスなし」"]
[]
[null,"２８．Ｕ値（入力根拠）はサッシ協ＨＰの場合は自動表記、計算/測定の場合は事業所が選択"]
[null,null,"サッシ協HP:建研HPの第三節　熱貫流率及び線熱貫流率による計算式からサッシ協会が算出した値による"]
[null,null,"計算/測定"," ：  ＪＩＳＡ４７１０、１４９２  ＩＳＯ１２５６７ による測定、又は、ＪＩＳＡ２１０２（ＷｉｎｄＥｙｅ）、"]
[null,null,null,"　　　ＩＳＯ１００７７による計算"]
[]
[null,"３０．η値（入力根拠）はサッシ協ＨＰの場合は自動表記、計算/測定の場合は事業所が選択"]
[null,null,"サッシ協HP：建研HPの第四節　日射熱取得率に記載の表をサッシ協会が転記したものによる"]
[null,null,"計算/測定","：JIS R 3106に定める測定"]
[null,"３９．一番厚いガラス厚は下記の厚さから事業所が選択"]
[null,null,"７、6.8、６、５、４、３"]
[null,"４０．遮音の性能根拠は事業所が選択"]
[null,null,"型式　：　型式認定"]
[null,null,"測定　：　"]
[]
[]
[null,"２６．付属部材は事業所が〇を選択"]
[null,"２７．熱貫流率はＵ値は１８．で仕様（ｻｯｼ協ＨＰ）を選択した場合は自動表記"]
[null,"　　　　　計算／測定を選択した場合は事業者が熱貫流率を入力する。"]
[null,"２９．日射熱取得率はη値は１８．で仕様（ｻｯｼＨＰ）を選択した場合は自動表記"]
[null,"　　　　　計算／測定を選択した場合は事業者が日射熱取得率を入力する。"]
[]
[null,"　　　※１４．開閉形式で、玄関ドア・引戸、勝手口ドア・引戸を選択した場合は、１８．記入区分で仕様を選択"]
[null,"　　　　　しても、１９、２０、２１、２２、２３、２４、２５は表記されないので、２７．熱貫流率と２９．日射熱取得率は、"]
[null,"　　　　　サッシメーカーのカタログを見て、ドア・引戸の商品名からサッシ協HPの建具仕様、ガラスの仕様を"]
[null,"　　　　　確認して、熱貫流率及び日射熱取得率を直接記入してください。"]
[]
[null,"３１．サッシメーカー名は事業所が入力"]
[null,"３１．サッシメーカー名"]
[null,null,"三協立山"]
[null,null,"不二サッシ"]
[null,null,"ＬＩＸＩＬ"]
[null,null,"ＹＫＫ ＡＰ"]
[null,null,"アルメタックス"]
[null,null,"エクセルシャノン"]
[null,"３２．シリーズ名又は記号は事業所が入力"]
[]
[null,"３７．防火対策（等級２…耐火２０分の防火設備）は事業所が該当するものに〇を選択"]
[null,"３８．遮音の該当する等級（３等級、２等級）を事業所が〇を選択"]
[null,"３９．遮音（一番厚いガラス厚）は事業所が厚さ（ｍｍ）を選択"]
[null,"４０．遮音（性能根拠）は事業所が選択"]
[null,"４１．防犯対策は該当するものに事業所が〇を選択"]

{"sheet":"マスターシート","index":4,"n_rows":394,"n_cols":6,"rows_kept":394,"cut":false,"hidden":true,"merged":[]}
["No20","No21","No22","No23","No24","No25"]
["建具仕様","ガラス種類","Ｌｏｗ－Ｅの有無","中空層種類","中空層厚み","建研ＨＰ"]
[1,"三層","ダブルLowE（日射取得型）","G","6×2",7]
[1,"三層","ダブルLowE（日射遮蔽型）","G","6×2",8]
[1,"三層","ダブルLowE（日射取得型）","G","7×2",5]
[1,"三層","ダブルLowE（日射遮蔽型）","G","7×2",6]
[1,"三層","ダブルLowE（日射取得型）","G","8×2",5]
[1,"三層","ダブルLowE（日射遮蔽型）","G","8×2",6]
[1,"三層","ダブルLowE（日射取得型）","G","9×2",5]
[1,"三層","ダブルLowE（日射遮蔽型）","G","9×2",6]
[1,"三層","ダブルLowE（日射取得型）","G","10×2",3]
[1,"三層","ダブルLowE（日射遮蔽型）","G","10×2",4]
[1,"三層","ダブルLowE（日射取得型）","G","11×2",3]
[1,"三層","ダブルLowE（日射遮蔽型）","G","11×2",4]
[1,"三層","ダブルLowE（日射取得型）","G","12×2",3]
[1,"三層","ダブルLowE（日射遮蔽型）","G","12×2",4]
[1,"三層","ダブルLowE（日射取得型）","G","13×2",1]
[1,"三層","ダブルLowE（日射遮蔽型）","G","13×2",2]
[1,"三層","ダブルLowE（日射取得型）","G","14×2",1]
[1,"三層","ダブルLowE（日射遮蔽型）","G","14×2",2]
[1,"三層","ダブルLowE（日射取得型）","G","15×2",1]
[1,"三層","ダブルLowE（日射遮蔽型）","G","15×2",2]
[1,"三層","ダブルLowE（日射取得型）","G","16×2",1]
[1,"三層","ダブルLowE（日射遮蔽型）","G","16×2",2]
[1,"三層","ダブルLowE（日射取得型）","A","6×2",15]
[1,"三層","ダブルLowE（日射遮蔽型）","A","6×2",16]
[1,"三層","ダブルLowE（日射取得型）","A","7×2",13]
[1,"三層","ダブルLowE（日射遮蔽型）","A","7×2",14]
[1,"三層","ダブルLowE（日射取得型）","A","8×2",13]
[1,"三層","ダブルLowE（日射遮蔽型）","A","8×2",14]
[1,"三層","ダブルLowE（日射取得型）","A","9×2",11]
[1,"三層","ダブルLowE（日射遮蔽型）","A","9×2",12]
[1,"三層","ダブルLowE（日射取得型）","A","10×2",11]
[1,"三層","ダブルLowE（日射遮蔽型）","A","10×2",12]
[1,"三層","ダブルLowE（日射取得型）","A","11×2",11]
[1,"三層","ダブルLowE（日射遮蔽型）","A","11×2",12]
[1,"三層","ダブルLowE（日射取得型）","A","12×2",11]
[1,"三層","ダブルLowE（日射遮蔽型）","A","12×2",12]
[1,"三層","ダブルLowE（日射取得型）","A","13×2",9]
[1,"三層","ダブルLowE（日射遮蔽型）","A","13×2",10]
[1,"三層","ダブルLowE（日射取得型）","A","14×2",9]
[1,"三層","ダブルLowE（日射遮蔽型）","A","14×2",10]
[1,"三層","ダブルLowE（日射取得型）","A","15×2",9]
[1,"三層","ダブルLowE（日射遮蔽型）","A","15×2",10]
[1,"三層","ダブルLowE（日射取得型）","A","16×2",9]
[1,"三層","ダブルLowE（日射遮蔽型）","A","16×2",10]
[1,"三層","LowE（日射取得型）","G","6×2",19]
[1,"三層","LowE（日射遮蔽型）","G","6×2",20]
[1,"三層","LowE（日射取得型）","G","7×2",19]
[1,"三層","LowE（日射遮蔽型）","G","7×2",20]
[1,"三層","LowE（日射取得型）","G","8×2",19]
[1,"三層","LowE（日射遮蔽型）","G","8×2",20]
[1,"三層","LowE（日射取得型）","G","9×2",19]
[1,"三層","LowE（日射遮蔽型）","G","9×2",20]
[1,"三層","LowE（日射取得型）","G","10×2",17]
[1,"三層","LowE（日射遮蔽型）","G","10×2",18]
[1,"三層","LowE（日射取得型）","G","11×2",17]
[1,"三層","LowE（日射遮蔽型）","G","11×2",18]
[1,"三層","LowE（日射取得型）","G","12×2",17]
[1,"三層","LowE（日射遮蔽型）","G","12×2",18]
[1,"三層","LowE（日射取得型）","G","13×2",17]
[1,"三層","LowE（日射遮蔽型）","G","13×2",18]
[1,"三層","LowE（日射取得型）","G","14×2",17]
[1,"三層","LowE（日射遮蔽型）","G","14×2",18]
[1,"三層","LowE（日射取得型）","G","15×2",17]
[1,"三層","LowE（日射遮蔽型）","G","15×2",18]
[1,"三層","LowE（日射取得型）","G","16×2",17]
[1,"三層","LowE（日射遮蔽型）","G","16×2",18]
[1,"三層","LowE（日射取得型）","A","6×2",27]
[1,"三層","LowE（日射遮蔽型）","A","6×2",28]
[1,"三層","LowE（日射取得型）","A","7×2",25]
[1,"三層","LowE（日射遮蔽型）","A","7×2",26]
[1,"三層","LowE（日射取得型）","A","8×2",25]
[1,"三層","LowE（日射遮蔽型）","A","8×2",26]
[1,"三層","LowE（日射取得型）","A","9×2",23]
[1,"三層","LowE（日射遮蔽型）","A","9×2",24]
[1,"三層","LowE（日射取得型）","A","10×2",23]
[1,"三層","LowE（日射遮蔽型）","A","10×2",24]
[1,"三層","LowE（日射取得型）","A","11×2",23]
[1,"三層","LowE（日射遮蔽型）","A","11×2",24]
[1,"三層","LowE（日射取得型）","A","12×2",23]
[1,"三層","LowE（日射遮蔽型）","A","12×2",24]
[1,"三層","LowE（日射取得型）","A","13×2",21]
[1,"三層","LowE（日射遮蔽型）","A","13×2",22]
[1,"三層","LowE（日射取得型）","A","14×2",21]
[1,"三層","LowE（日射遮蔽型）","A","14×2",22]
[1,"三層","LowE（日射取得型）","A","15×2",21]
[1,"三層","LowE（日射遮蔽型）","A","15×2",22]
[1,"三層","LowE（日射取得型）","A","16×2",21]
[1,"三層","LowE（日射遮蔽型）","A","16×2",22]
[1,"三層","無し","A","6×2",30]
[1,"三層","無し","A","7×2",30]
[1,"三層","無し","A","8×2",30]
[1,"三層","無し","A","9×2",30]
[1,"三層","無し","A","10×2",30]
[1,"三層","無し","A","11×2",30]
[1,"三層","無し","A","12×2",30]
[1,"三層","無し","A","13×2",29]
[1,"三層","無し","A","14×2",29]
[1,"三層","無し","A","15×2",29]
[1,"三層","無し","A","16×2",29]
[1,"複層","LowE（日射取得型）","G",4,35]
[1,"複層","LowE（日射遮蔽型）","G",4,36]
[1,"複層","LowE（日射取得型）","G",5,35]
[1,"複層","LowE（日射遮蔽型）","G",5,36]
[1,"複層","LowE（日射取得型）","G",6,35]
[1,"複層","LowE（日射遮蔽型）","G",6,36]
[1,"複層","LowE（日射取得型）","G",7,35]
[1,"複層","LowE（日射遮蔽型）","G",7,36]
[1,"複層","LowE（日射取得型）","G",8,33]
[1,"複層","LowE（日射遮蔽型）","G",8,34]
[1,"複層","LowE（日射取得型）","G",9,33]
[1,"複層","LowE（日射遮蔽型）","G",9,34]
[1,"複層","LowE（日射取得型）","G",10,31]
[1,"複層","LowE（日射遮蔽型）","G",10,32]
[1,"複層","LowE（日射取得型）","G",11,31]
[1,"複層","LowE（日射遮蔽型）","G",11,32]
[1,"複層","LowE（日射取得型）","G",12,31]
[1,"複層","LowE（日射遮蔽型）","G",12,32]
[1,"複層","LowE（日射取得型）","G",13,31]
[1,"複層","LowE（日射遮蔽型）","G",13,32]
[1,"複層","LowE（日射取得型）","G",14,31]
[1,"複層","LowE（日射遮蔽型）","G",14,32]
[1,"複層","LowE（日射取得型）","G",15,31]
[1,"複層","LowE（日射遮蔽型）","G",15,32]
[1,"複層","LowE（日射取得型）","G",16,31]
[1,"複層","LowE（日射遮蔽型）","G",16,32]
[1,"複層","LowE（日射取得型）","A",4,41]
[1,"複層","LowE（日射遮蔽型）","A",4,42]
[1,"複層","LowE（日射取得型）","A",5,41]
[1,"複層","LowE（日射遮蔽型）","A",5,42]
[1,"複層","LowE（日射取得型）","A",6,41]
[1,"複層","LowE（日射遮蔽型）","A",6,42]
[1,"複層","LowE（日射取得型）","A",7,41]
[1,"複層","LowE（日射遮蔽型）","A",7,42]
[1,"複層","LowE（日射取得型）","A",8,41]
[1,"複層","LowE（日射遮蔽型）","A",8,42]
[1,"複層","LowE（日射取得型）","A",9,41]
[1,"複層","LowE（日射遮蔽型）","A",9,42]
[1,"複層","LowE（日射取得型）","A",10,41]
[1,"複層","LowE（日射遮蔽型）","A",10,42]
[1,"複層","LowE（日射取得型）","A",11,39]
[1,"複層","LowE（日射遮蔽型）","A",11,40]
[1,"複層","LowE（日射取得型）","A",12,39]
[1,"複層","LowE（日射遮蔽型）","A",12,40]
[7,"複層","LowE（日射取得型）","A",13,39]
[1,"複層","LowE（日射遮蔽型）","A",13,40]
[1,"複層","LowE（日射取得型）","A",14,37]
[1,"複層","LowE（日射遮蔽型）","A",14,38]
[1,"複層","LowE（日射取得型）","A",15,37]
[1,"複層","LowE（日射遮蔽型）","A",15,38]
[1,"複層","LowE（日射取得型）","A",16,37]
[1,"複層","LowE（日射遮蔽型）","A",16,38]
[1,"複層","無し","A",6,42]
[1,"複層","無し","A",7,42]
[1,"複層","無し","A",8,42]
[1,"複層","無し","A",9,42]
[1,"複層","無し","A",10,42]
[1,"複層","無し","A",11,42]
[1,"複層","無し","A",12,42]
[1,"複層","無し","A",13,43]
[1,"複層","無し","A",14,43]
[1,"複層","無し","A",15,43]
[1,"複層","無し","A",16,43]
[1,"単板","無し","N","単板",45]
[2,"三層","ダブルLowE（日射取得型）","G","6×2",50]
[2,"三層","ダブルLowE（日射遮蔽型）","G","6×2",51]
[2,"三層","ダブルLowE（日射取得型）","G","7×2",50]
[2,"三層","ダブルLowE（日射遮蔽型）","G","7×2",51]
[2,"三層","ダブルLowE（日射取得型）","G","8×2",48]
[2,"三層","ダブルLowE（日射遮蔽型）","G","8×2",49]
[2,"三層","ダブルLowE（日射取得型）","G","9×2",48]
[2,"三層","ダブルLowE（日射遮蔽型）","G","9×2",49]
[2,"三層","ダブルLowE（日射取得型）","G","10×2",48]
[2,"三層","ダブルLowE（日射遮蔽型）","G","10×2",49]
[2,"三層","ダブルLowE（日射取得型）","G","11×2",48]
[2,"三層","ダブルLowE（日射遮蔽型）","G","11×2",49]
[2,"三層","ダブルLowE（日射取得型）","G","12×2",46]
[2,"三層","ダブルLowE（日射遮蔽型）","G","12×2",47]
[2,"三層","ダブルLowE（日射取得型）","G","13×2",46]
[2,"三層","ダブルLowE（日射遮蔽型）","G","13×2",47]
[2,"三層","ダブルLowE（日射取得型）","G","14×2",46]
[2,"三層","ダブルLowE（日射遮蔽型）","G","14×2",47]
[2,"三層","ダブルLowE（日射取得型）","G","15×2",46]
[2,"三層","ダブルLowE（日射遮蔽型）","G","15×2",47]
[2,"三層","ダブルLowE（日射取得型）","G","16×2",46]
[2,"三層","ダブルLowE（日射遮蔽型）","G","16×2",47]
[2,"三層","ダブルLowE（日射取得型）","A","6×2",58]
[2,"三層","ダブルLowE（日射遮蔽型）","A","6×2",59]
[2,"三層","ダブルLowE（日射取得型）","A","7×2",58]
[2,"三層","ダブルLowE（日射遮蔽型）","A","7×2",59]
[2,"三層","ダブルLowE（日射取得型）","A","8×2",56]
[2,"三層","ダブルLowE（日射遮蔽型）","A","8×2",57]
[2,"三層","ダブルLowE（日射取得型）","A","9×2",56]
[2,"三層","ダブルLowE（日射遮蔽型）","A","9×2",57]
[2,"三層","ダブルLowE（日射取得型）","A","10×2",54]
[2,"三層","ダブルLowE（日射遮蔽型）","A","10×2",55]
[2,"三層","ダブルLowE（日射取得型）","A","11×2",54]
[2,"三層","ダブルLowE（日射遮蔽型）","A","11×2",55]
[2,"三層","ダブルLowE（日射取得型）","A","12×2",54]
[2,"三層","ダブルLowE（日射遮蔽型）","A","12×2",55]
[2,"三層","ダブルLowE（日射取得型）","A","13×2",54]
[2,"三層","ダブルLowE（日射遮蔽型）","A","13×2",55]
[2,"三層","ダブルLowE（日射取得型）","A","14×2",54]
[2,"三層","ダブルLowE（日射遮蔽型）","A","14×2",55]
[2,"三層","ダブルLowE（日射取得型）","A","15×2",54]
[2,"三層","ダブルLowE（日射遮蔽型）","A","15×2",55]
[2,"三層","ダブルLowE（日射取得型）","A","16×2",52]
[2,"三層","ダブルLowE（日射遮蔽型）","A","16×2",53]
[2,"三層","LowE（日射取得型）","G","6×2",64]
[2,"三層","LowE（日射遮蔽型）","G","6×2",65]
[2,"三層","LowE（日射取得型）","G","7×2",64]
[2,"三層","LowE（日射遮蔽型）","G","7×2",65]
[2,"三層","LowE（日射取得型）","G","8×2",64]
[2,"三層","LowE（日射遮蔽型）","G","8×2",65]
[2,"三層","LowE（日射取得型）","G","9×2",62]
[2,"三層","LowE（日射遮蔽型）","G","9×2",63]
[2,"三層","LowE（日射取得型）","G","10×2",62]
[2,"三層","LowE（日射遮蔽型）","G","10×2",63]
[2,"三層","LowE（日射取得型）","G","11×2",62]
[2,"三層","LowE（日射遮蔽型）","G","11×2",63]
[2,"三層","LowE（日射取得型）","G","12×2",60]
[2,"三層","LowE（日射遮蔽型）","G","12×2",61]
[2,"三層","LowE（日射取得型）","G","13×2",60]
[2,"三層","LowE（日射遮蔽型）","G","13×2",61]
[2,"三層","LowE（日射取得型）","G","14×2",60]
[2,"三層","LowE（日射遮蔽型）","G","14×2",61]
[2,"三層","LowE（日射取得型）","G","15×2",60]
[2,"三層","LowE（日射遮蔽型）","G","15×2",61]
[2,"三層","LowE（日射取得型）","G","16×2",60]
[2,"三層","LowE（日射遮蔽型）","G","16×2",61]
[2,"三層","LowE（日射取得型）","A","6×2",70]
[2,"三層","LowE（日射遮蔽型）","A","6×2",71]
[2,"三層","LowE（日射取得型）","A","7×2",70]
[2,"三層","LowE（日射遮蔽型）","A","7×2",71]
[2,"三層","LowE（日射取得型）","A","8×2",70]
[2,"三層","LowE（日射遮蔽型）","A","8×2",71]
[2,"三層","LowE（日射取得型）","A","9×2",70]
[2,"三層","LowE（日射遮蔽型）","A","9×2",71]
[2,"三層","LowE（日射取得型）","A","10×2",70]
[2,"三層","LowE（日射遮蔽型）","A","10×2",71]
[2,"三層","LowE（日射取得型）","A","11×2",70]
[2,"三層","LowE（日射遮蔽型）","A","11×2",71]
[2,"三層","LowE（日射取得型）","A","12×2",68]
[2,"三層","LowE（日射遮蔽型）","A","12×2",69]
[2,"三層","LowE（日射取得型）","A","13×2",68]
[2,"三層","LowE（日射遮蔽型）","A","13×2",69]
[2,"三層","LowE（日射取得型）","A","14×2",68]
[2,"三層","LowE（日射遮蔽型）","A","14×2",69]
[2,"三層","LowE（日射取得型）","A","15×2",68]
[2,"三層","LowE（日射遮蔽型）","A","15×2",69]
[2,"三層","LowE（日射取得型）","A","16×2",66]
[2,"三層","LowE（日射遮蔽型）","A","16×2",67]
[2,"三層","無し","A","6×2",73]
[2,"三層","無し","A","7×2",72]
[2,"三層","無し","A","8×2",72]
[2,"三層","無し","A","9×2",72]
[2,"三層","無し","A","10×2",72]
[2,"三層","無し","A","11×2",72]
[2,"三層","無し","A","12×2",72]
[2,"三層","無し","A","13×2",72]
[2,"三層","無し","A","14×2",72]
[2,"三層","無し","A","15×2",72]
[2,"三層","無し","A","16×2",72]
[2,"複層","LowE（日射取得型）","G",4,76]
[2,"複層","LowE（日射遮蔽型）","G",4,77]
[2,"複層","LowE（日射取得型）","G",5,76]
[2,"複層","LowE（日射遮蔽型）","G",5,77]
[2,"複層","LowE（日射取得型）","G",6,76]
[2,"複層","LowE（日射遮蔽型）","G",6,77]
[2,"複層","LowE（日射取得型）","G",7,76]
[2,"複層","LowE（日射遮蔽型）","G",7,77]
[2,"複層","LowE（日射取得型）","G",8,76]
[2,"複層","LowE（日射遮蔽型）","G",8,77]
[2,"複層","LowE（日射取得型）","G",9,76]
[2,"複層","LowE（日射遮蔽型）","G",9,77]
[2,"複層","LowE（日射取得型）","G",10,76]
[2,"複層","LowE（日射遮蔽型）","G",10,77]
[2,"複層","LowE（日射取得型）","G",11,76]
[2,"複層","LowE（日射遮蔽型）","G",11,77]
[2,"複層","LowE（日射取得型）","G",12,76]
[2,"複層","LowE（日射遮蔽型）","G",12,77]
[2,"複層","LowE（日射取得型）","G",13,76]
[2,"複層","LowE（日射遮蔽型）","G",13,77]
[2,"複層","LowE（日射取得型）","G",14,74]
[2,"複層","LowE（日射遮蔽型）","G",14,75]
[2,"複層","LowE（日射取得型）","G",15,74]
[2,"複層","LowE（日射遮蔽型）","G",15,75]
[2,"複層","LowE（日射取得型）","G",16,74]
[2,"複層","LowE（日射遮蔽型）","G",16,75]
[2,"複層","LowE（日射取得型）","A",4,80]
[2,"複層","LowE（日射遮蔽型）","A",4,81]
[2,"複層","LowE（日射取得型）","A",5,80]
[2,"複層","LowE（日射遮蔽型）","A",5,81]
[2,"複層","LowE（日射取得型）","A",6,80]
[2,"複層","LowE（日射遮蔽型）","A",6,81]
[2,"複層","LowE（日射取得型）","A",7,80]
[2,"複層","LowE（日射遮蔽型）","A",7,81]
[2,"複層","LowE（日射取得型）","A",8,80]
[2,"複層","LowE（日射遮蔽型）","A",8,81]
[2,"複層","LowE（日射取得型）","A",9,78]
[2,"複層","LowE（日射遮蔽型）","A",9,79]
[2,"複層","LowE（日射取得型）","A",10,78]
[2,"複層","LowE（日射遮蔽型）","A",10,79]
[2,"複層","LowE（日射取得型）","A",11,78]
[2,"複層","LowE（日射遮蔽型）","A",11,79]
[2,"複層","LowE（日射取得型）","A",12,78]
[2,"複層","LowE（日射遮蔽型）","A",12,79]
[2,"複層","LowE（日射取得型）","A",13,78]
[2,"複層","LowE（日射遮蔽型）","A",13,79]
[2,"複層","LowE（日射取得型）","A",14,78]
[2,"複層","LowE（日射遮蔽型）","A",14,79]
[2,"複層","LowE（日射取得型）","A",15,78]
[2,"複層","LowE（日射遮蔽型）","A",15,79]
[2,"複層","LowE（日射取得型）","A",16,78]
[2,"複層","LowE（日射遮蔽型）","A",16,79]
[2,"複層","無し","A",6,83]
[2,"複層","無し","A",7,83]
[2,"複層","無し","A",8,83]
[2,"複層","無し","A",9,83]
[2,"複層","無し","A",10,83]
[2,"複層","無し","A",11,82]
[2,"複層","無し","A",12,82]
[2,"複層","無し","A",13,82]
[2,"複層","無し","A",14,82]
[2,"複層","無し","A",15,82]
[2,"複層","無し","A",16,82]
[2,"単板","無し","N","単板",84]
[3,"複層","LowE（日射取得型）","G",4,87]
[3,"複層","LowE（日射遮蔽型）","G",4,88]
[3,"複層","LowE（日射取得型）","G",5,87]
[3,"複層","LowE（日射遮蔽型）","G",5,88]
[3,"複層","LowE（日射取得型）","G",6,87]
[3,"複層","LowE（日射遮蔽型）","G",6,88]
[3,"複層","LowE（日射取得型）","G",7,87]
[3,"複層","LowE（日射遮蔽型）","G",7,88]
[3,"複層","LowE（日射取得型）","G",8,87]
[3,"複層","LowE（日射遮蔽型）","G",8,88]
[3,"複層","LowE（日射取得型）","G",9,87]
[3,"複層","LowE（日射遮蔽型）","G",9,88]
[3,"複層","LowE（日射取得型）","G",10,85]
[3,"複層","LowE（日射遮蔽型）","G",10,86]
[3,"複層","LowE（日射取得型）","G",11,85]
[3,"複層","LowE（日射遮蔽型）","G",11,86]
[3,"複層","LowE（日射取得型）","G",12,85]
[3,"複層","LowE（日射遮蔽型）","G",12,86]
[3,"複層","LowE（日射取得型）","G",13,85]
[3,"複層","LowE（日射遮蔽型）","G",13,86]
[3,"複層","LowE（日射取得型）","G",14,85]
[3,"複層","LowE（日射遮蔽型）","G",14,86]
[3,"複層","LowE（日射取得型）","G",15,85]
[3,"複層","LowE（日射遮蔽型）","G",15,86]
[3,"複層","LowE（日射取得型）","G",16,85]
[3,"複層","LowE（日射遮蔽型）","G",16,86]
[3,"複層","LowE（日射取得型）","A",4,93]
[3,"複層","LowE（日射遮蔽型）","A",4,94]
[3,"複層","LowE（日射取得型）","A",5,93]
[3,"複層","LowE（日射遮蔽型）","A",5,94]
[3,"複層","LowE（日射取得型）","A",6,93]
[3,"複層","LowE（日射遮蔽型）","A",6,94]
[3,"複層","LowE（日射取得型）","A",7,91]
[3,"複層","LowE（日射遮蔽型）","A",7,92]
[3,"複層","LowE（日射取得型）","A",8,91]
[3,"複層","LowE（日射遮蔽型）","A",8,92]
[3,"複層","LowE（日射取得型）","A",9,91]
[3,"複層","LowE（日射遮蔽型）","A",9,92]
[3,"複層","LowE（日射取得型）","A",10,91]
[3,"複層","LowE（日射遮蔽型）","A",10,92]
[3,"複層","LowE（日射取得型）","A",11,91]
[3,"複層","LowE（日射遮蔽型）","A",11,92]
[3,"複層","LowE（日射取得型）","A",12,91]
[3,"複層","LowE（日射遮蔽型）","A",12,92]
[3,"複層","LowE（日射取得型）","A",13,91]
[3,"複層","LowE（日射遮蔽型）","A",13,92]
[3,"複層","LowE（日射取得型）","A",14,89]
[3,"複層","LowE（日射遮蔽型）","A",14,90]
[3,"複層","LowE（日射取得型）","A",15,89]
[3,"複層","LowE（日射遮蔽型）","A",15,90]
[3,"複層","LowE（日射取得型）","A",16,89]
[3,"複層","LowE（日射遮蔽型）","A",16,90]
[3,"複層","無し","A",4,96]
[3,"複層","無し","A",5,96]
[3,"複層","無し","A",6,96]
[3,"複層","無し","A",7,96]
[3,"複層","無し","A",8,95]
[3,"複層","無し","A",9,95]
[3,"複層","無し","A",10,95]
[3,"複層","無し","A",11,95]
[3,"複層","無し","A",12,95]
[3,"複層","無し","A",13,95]
[3,"複層","無し","A",14,95]
[3,"複層","無し","A",15,95]
[3,"複層","無し","A",16,95]
[3,"単板","単板","N","単板",97]

{"sheet":"DATA BASE","index":5,"n_rows":394,"n_cols":10,"rows_kept":394,"cut":false,"hidden":true,"merged":[[0,7,0,9]]}
["No20","No21","No22","No23","No24","No25","No27","No29"]
["建具仕様","ガラス種類","Ｌｏｗ－Ｅの有無","中空層種類","中空層厚み","建建ＨＰ","Ｕ値","η値","和障子","外付け\nブラインド"]
[1,"三層","ダブルLowE（日射取得型）","G","6×2",7,2.15,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","6×2",8,2.15,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","7×2",5,1.9,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","7×2",6,1.9,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","8×2",5,1.9,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","8×2",6,1.9,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","9×2",5,1.9,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","9×2",6,1.9,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","10×2",3,1.7,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","10×2",4,1.7,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","11×2",3,1.7,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","11×2",4,1.7,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","12×2",3,1.7,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","12×2",4,1.7,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","13×2",1,1.6,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","13×2",2,1.6,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","14×2",1,1.6,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","14×2",2,1.6,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","15×2",1,1.6,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","15×2",2,1.6,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","G","16×2",1,1.6,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","G","16×2",2,1.6,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","6×2",15,2.33,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","6×2",16,2.33,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","7×2",13,2.15,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","7×2",14,2.15,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","8×2",13,2.15,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","8×2",14,2.15,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","9×2",11,1.9,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","9×2",12,1.9,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","10×2",11,1.9,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","10×2",12,1.9,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","11×2",11,1.9,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","11×2",12,1.9,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","12×2",11,1.9,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","12×2",12,1.9,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","13×2",9,1.7,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","13×2",10,1.7,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","14×2",9,1.7,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","14×2",10,1.7,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","15×2",9,1.7,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","15×2",10,1.7,0.24,0.16,0.06]
[1,"三層","ダブルLowE（日射取得型）","A","16×2",9,1.7,0.39,0.24,0.09]
[1,"三層","ダブルLowE（日射遮蔽型）","A","16×2",10,1.7,0.24,0.16,0.06]
[1,"三層","LowE（日射取得型）","G","6×2",19,2.15,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","6×2",20,2.15,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","7×2",19,2.15,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","7×2",20,2.15,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","8×2",19,2.15,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","8×2",20,2.15,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","9×2",19,2.15,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","9×2",20,2.15,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","10×2",17,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","10×2",18,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","11×2",17,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","11×2",18,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","12×2",17,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","12×2",18,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","13×2",17,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","13×2",18,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","14×2",17,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","14×2",18,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","15×2",17,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","15×2",18,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","G","16×2",17,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","G","16×2",18,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","6×2",27,2.91,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","6×2",28,2.91,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","7×2",25,2.33,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","7×2",26,2.33,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","8×2",25,2.33,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","8×2",26,2.33,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","9×2",23,2.15,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","9×2",24,2.15,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","10×2",23,2.15,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","10×2",24,2.15,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","11×2",23,2.15,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","11×2",24,2.15,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","12×2",23,2.15,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","12×2",24,2.15,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","13×2",21,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","13×2",22,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","14×2",21,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","14×2",22,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","15×2",21,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","15×2",22,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","LowE（日射取得型）","A","16×2",21,1.9,0.42,0.27,0.1]
[1,"三層","LowE（日射遮蔽型）","A","16×2",22,1.9,0.27,0.18,7.0000000000000007E-2]
[1,"三層","無し","A","6×2",30,2.91,0.52,0.27,0.13]
[1,"三層","無し","A","7×2",30,2.91,0.52,0.27,0.13]
[1,"三層","無し","A","8×2",30,2.91,0.52,0.27,0.13]
[1,"三層","無し","A","9×2",30,2.91,0.52,0.27,0.13]
[1,"三層","無し","A","10×2",30,2.91,0.52,0.27,0.13]
[1,"三層","無し","A","11×2",30,2.91,0.52,0.27,0.13]
[1,"三層","無し","A","12×2",30,2.91,0.52,0.27,0.13]
[1,"三層","無し","A","13×2",29,2.33,0.52,0.27,0.13]
[1,"三層","無し","A","14×2",29,2.33,0.52,0.27,0.13]
[1,"三層","無し","A","15×2",29,2.33,0.52,0.27,0.13]
[1,"三層","無し","A","16×2",29,2.33,0.52,0.27,0.13]
[1,"複層","LowE（日射取得型）","G",4,35,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",4,36,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",5,35,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",5,36,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",6,35,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",6,36,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",7,35,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",7,36,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",8,33,2.33,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",8,34,2.33,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",9,33,2.33,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",9,34,2.33,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",10,31,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",10,32,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",11,31,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",11,32,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",12,31,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",12,32,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",13,31,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",13,32,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",14,31,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",14,32,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",15,31,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",15,32,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","G",16,31,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","G",16,32,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",4,41,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",4,42,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",5,41,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",5,42,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",6,41,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",6,42,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",7,41,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",7,42,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",8,41,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",8,42,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",9,41,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",9,42,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",10,41,2.91,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",10,42,2.91,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",11,39,2.33,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",11,40,2.33,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",12,39,2.33,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",12,40,2.33,0.28999999999999998,0.19,0.08]
[7,"複層","LowE（日射取得型）","A",13,39,2.33,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",13,40,2.33,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",14,37,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",14,38,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",15,37,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",15,38,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","LowE（日射取得型）","A",16,37,2.15,0.46,0.27,0.11]
[1,"複層","LowE（日射遮蔽型）","A",16,38,2.15,0.28999999999999998,0.19,0.08]
[1,"複層","無し","A",6,42,3.49,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",7,42,3.49,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",8,42,3.49,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",9,42,3.49,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",10,42,3.49,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",11,42,3.49,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",12,42,3.49,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",13,43,2.91,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",14,43,2.91,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",15,43,2.91,0.56999999999999995,0.27,0.12]
[1,"複層","無し","A",16,43,2.91,0.56999999999999995,0.27,0.12]
[1,"単板","無し","N","単板",45,6.51,0.63,0.27,0.14000000000000001]
[2,"三層","ダブルLowE（日射取得型）","G","6×2",50,2.33,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","6×2",51,2.33,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","7×2",50,2.33,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","7×2",51,2.33,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","8×2",48,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","8×2",49,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","9×2",48,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","9×2",49,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","10×2",48,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","10×2",49,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","11×2",48,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","11×2",49,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","12×2",46,1.9,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","12×2",47,1.9,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","13×2",46,1.9,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","13×2",47,1.9,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","14×2",46,1.9,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","14×2",47,1.9,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","15×2",46,1.9,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","15×2",47,1.9,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","G","16×2",46,1.9,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","G","16×2",47,1.9,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","6×2",58,2.91,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","6×2",59,2.91,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","7×2",58,2.91,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","7×2",59,2.91,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","8×2",56,2.33,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","8×2",57,2.33,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","9×2",56,2.33,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","9×2",57,2.33,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","10×2",54,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","10×2",55,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","11×2",54,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","11×2",55,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","12×2",54,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","12×2",55,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","13×2",54,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","13×2",55,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","14×2",54,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","14×2",55,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","15×2",54,2.15,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","15×2",55,2.15,0.26,0.18,0.06]
[2,"三層","ダブルLowE（日射取得型）","A","16×2",52,1.9,0.43,0.27,0.1]
[2,"三層","ダブルLowE（日射遮蔽型）","A","16×2",53,1.9,0.26,0.18,0.06]
[2,"三層","LowE（日射取得型）","G","6×2",64,2.91,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","6×2",65,2.91,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","7×2",64,2.91,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","7×2",65,2.91,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","8×2",64,2.91,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","8×2",65,2.91,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","9×2",62,2.33,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","9×2",63,2.33,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","10×2",62,2.33,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","10×2",63,2.33,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","11×2",62,2.33,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","11×2",63,2.33,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","12×2",60,2.15,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","12×2",61,2.15,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","13×2",60,2.15,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","13×2",61,2.15,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","14×2",60,2.15,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","14×2",61,2.15,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","15×2",60,2.15,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","15×2",61,2.15,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","G","16×2",60,2.15,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","G","16×2",61,2.15,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","6×2",70,2.91,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","6×2",71,2.91,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","7×2",70,2.91,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","7×2",71,2.91,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","8×2",70,2.91,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","8×2",71,2.91,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","9×2",70,2.91,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","9×2",71,2.91,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","10×2",70,2.91,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","10×2",71,2.91,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","11×2",70,2.91,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","11×2",71,2.91,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","12×2",68,2.33,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","12×2",69,2.33,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","13×2",68,2.33,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","13×2",69,2.33,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","14×2",68,2.33,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","14×2",69,2.33,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","15×2",68,2.33,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","15×2",69,2.33,0.3,0.2,0.08]
[2,"三層","LowE（日射取得型）","A","16×2",66,2.15,0.47,0.3,0.11]
[2,"三層","LowE（日射遮蔽型）","A","16×2",67,2.15,0.3,0.2,0.08]
[2,"三層","無し","A","6×2",73,3.49,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","7×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","8×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","9×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","10×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","11×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","12×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","13×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","14×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","15×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"三層","無し","A","16×2",72,2.91,0.57999999999999996,0.3,0.14000000000000001]
[2,"複層","LowE（日射取得型）","G",4,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",4,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",5,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",5,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",6,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",6,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",7,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",7,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",8,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",8,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",9,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",9,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",10,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",10,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",11,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",11,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",12,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",12,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",13,76,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",13,77,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",14,74,2.33,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",14,75,2.33,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",15,74,2.33,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",15,75,2.33,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","G",16,74,2.33,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","G",16,75,2.33,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",4,80,3.49,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",4,81,3.49,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",5,80,3.49,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",5,81,3.49,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",6,80,3.49,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",6,81,3.49,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",7,80,3.49,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",7,81,3.49,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",8,80,3.49,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",8,81,3.49,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",9,78,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",9,79,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",10,78,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",10,79,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",11,78,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",11,79,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",12,78,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",12,79,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",13,78,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",13,79,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",14,78,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",14,79,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",15,78,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",15,79,2.91,0.32,0.21,0.09]
[2,"複層","LowE（日射取得型）","A",16,78,2.91,0.51,0.3,0.12]
[2,"複層","LowE（日射遮蔽型）","A",16,79,2.91,0.32,0.21,0.09]
[2,"複層","無し","A",6,83,4.07,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",7,83,4.07,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",8,83,4.07,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",9,83,4.07,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",10,83,4.07,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",11,82,3.49,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",12,82,3.49,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",13,82,3.49,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",14,82,3.49,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",15,82,3.49,0.63,0.3,0.14000000000000001]
[2,"複層","無し","A",16,82,3.49,0.63,0.3,0.14000000000000001]
[2,"単板","無し","N","単板",84,6.51,0.7,0.3,0.15]
[3,"複層","LowE（日射取得型）","G",4,87,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",4,88,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",5,87,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",5,88,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",6,87,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",6,88,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",7,87,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",7,88,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",8,87,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",8,88,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",9,87,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",9,88,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",10,85,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",10,86,2.91,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",11,85,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",11,86,2.91,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",12,85,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",12,86,2.91,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",13,85,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",13,86,2.91,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",14,85,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",14,86,2.91,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",15,85,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",15,86,2.91,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","G",16,85,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","G",16,86,2.91,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",4,93,4.07,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",4,94,4.07,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",5,93,4.07,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",5,94,4.07,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",6,93,4.07,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",6,94,4.07,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",7,91,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",7,92,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",8,91,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",8,92,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",9,91,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",9,92,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",10,91,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",10,92,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",11,91,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",11,92,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",12,91,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",12,92,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",13,91,3.49,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",13,92,3.49,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",14,89,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",14,90,2.91,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",15,89,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",15,90,2.91,0.32,0.21,0.09]
[3,"複層","LowE（日射取得型）","A",16,89,2.91,0.51,0.3,0.12]
[3,"複層","LowE（日射遮蔽型）","A",16,90,2.91,0.32,0.21,0.09]
[3,"複層","無し","A",4,96,4.6500000000000004,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",5,96,4.6500000000000004,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",6,96,4.6500000000000004,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",7,96,4.6500000000000004,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",8,95,4.07,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",9,95,4.07,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",10,95,4.07,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",11,95,4.07,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",12,95,4.07,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",13,95,4.07,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",14,95,4.07,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",15,95,4.07,0.63,0.3,0.14000000000000001]
[3,"複層","無し","A",16,95,4.07,0.63,0.3,0.14000000000000001]
[3,"単板","単板","N","単板",97,6.51,0.7,0.3,0.15]

{"sheet":"建具仕様番号","index":6,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":true,"merged":[]}
["樹脂",1]
["アルミ樹脂複合",2]
["アルミ熱遮断構造",3]
["アルミＰＧ",3]
["アルミＳＧ",3]
["アルミＳＧ＋樹脂内窓",4]
["木製",1]
["アルミ木複合",2]
["ドア１",7]
["ドア２",7]
["ドア３",7]
["ドア４",7]